{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Template"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Template","index":0,"n_rows":5,"n_cols":52,"rows_kept":5,"cut":false,"hidden":false,"merged":[[2,0,2,3]]}
[]
["D45EuDN7/1.10","zoneease_1.3","zh","si",null,"18","15","121","114","115","117","118","119","120","167","4","2","5","6","7","24","25","26","60","61","27","28","105","106","29","150","151","152","11","12","103","124","125","126","138","139","140","141","145","146","127","128","129","130","131","132","133"]
["场地",null,null,null,null,"控制","","","BACnet","","","","","","","整体","","","","","","","","","","","","","","","","","","标定VAV箱","","","控制总线选项","","","PoE设定","","","","","","BACnet IP设定","","","","Modbus TCP设定","",""]
["建筑","地板","房间","方框标识码",null,"最小风量","最大风量","制热最大风量","RS485-波特率","RS485-地址","BACnet-编号","BACnet-对象名","BACnet-位置","BACnet-描述","BACnet-中继编码","应用编码","增强时间","经济模式制热设定","经济模式制冷设定","关闭模式风门开度","温控器温度显示","温控器权限","温控器商标显示","房间温度高限","房间温度低限","CO2低限","CO2高限","风门同步开度","上电模式","占空功能","房间单元温度单位","AI传感器配置","压力相关模式","额定压差","额定风量","旋转方向","执行器类型","RS485","以太网IP","固定IP","主地址","子网掩码","网关地址","DNS1地址","DNS2地址","TCP端口","外部设备","IP广播管理设备","生存时间","地址","TCP端口","时限"]
[null,null,null,null,null,0.0,0.0,0.0,"2",2.0,23.0,"ZoneEase VAV","Location","ZoneEase VAV Room Comfort Cnt. Solution incl. VAV and CO2 Cnt.",1.0,"1",10.0,4.0,4.0,"1","1","1","1",28.0,18.0,0.0,2000.0,"1","2","0","0","2","1",null,null,"0","0","1","0","0","192.168.1.10","255.255.255.0","192.168.1.1","0.0.0.0","0.0.0.0",47808.0,"0","127.0.0.1",30.0,1.0,502.0,3.0]