{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Template"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Template","index":0,"n_rows":5,"n_cols":52,"rows_kept":5,"cut":false,"hidden":false,"merged":[[2,0,2,3]]}
[]
["D45EuDN7/1.10","zoneease_1.3","en","uscs",null,"18","15","121","114","115","117","118","119","120","167","4","2","5","6","7","24","25","26","60","61","27","28","105","106","29","150","151","152","11","12","103","124","125","126","138","139","140","141","145","146","127","128","129","130","131","132","133"]
["Site",null,null,null,null,"Control","","","BACnet","","","","","","","Global","","","","","","","","","","","","","","","","","","Box Calibration","","","BMS-Bus Selection","","","PoE Settings","","","","","","BACnet IP Settings","","","","Modbus TCP Settings","",""]
["Building","Floor","Room","Box ID",null,"V'min [cfm]","V'max Cooling [cfm]","V'max Heating [cfm]","Baudrate","Address","Instance Number","Object Name","Location","Description","BACnet Trunk No.","Application Number","Boost Mode Time [min]","Eco Mode Heating Shift [Δ°F]","Eco Mode Cooling Shift [Δ°F]","Off Mode Damper Pos","Room Unit Display","Room Unit Rights","Room Unit Logo","Setpoint Temp High Lim [°F]","Setpoint Temp Low Lim [°F]","CO2 Sensor min Limit [ppm]","CO2 Sensor max Limit [ppm]","Damper Sync Position","Power On Mode","Occupancy Sensor","Room Unit Temp. Unit","AI sensor configuration","Pressure dependence mode","Δp@V'nom [inWC]","V'nom [cfm]","Rotation Direction","Actuator Type","RS485","Ethernet IP","Static IP","Host Address","Subnet Network Mask","Gateway Address","DNS1 Address","DNS2 Address","TCP Port","Foreign Device","IP BBDM","Time-To-Live","Address","Modbus TCP Port","Modbus Time Limit"]
[null,null,null,null,null,0.0,0.0,0.0,"2",2.0,23.0,"ZoneEase VAV","Location","ZoneEase VAV Room Comfort Cnt. Solution incl. VAV and CO2 Cnt.",1.0,"1",10.0,7.2,7.2,"1","1","1","1",82.4,64.4,0.0,2000.0,"1","2","0","1","2","1",null,null,"0","0","1","0","0","192.168.1.10","255.255.255.0","192.168.1.1","0.0.0.0","0.0.0.0",47808.0,"0","127.0.0.1",30.0,1.0,502.0,3.0]